# G. Uniform Fuels and Automotive Lubricants Regulation

**Table of Contents**

## Section Page

[Section 1. Definitions 187](#_bookmark1)

* 1. [ASTM (ASTM International) 187](#_bookmark2)
  2. [Antiknock Index (AKI) 187](#_bookmark3)
  3. [Automatic Transmission Fluid 187](#_bookmark4)
  4. [Automotive Fuel Rating 187](#_bookmark5)
  5. [Automotive Gasoline, Automotive Gasoline-Oxygenate Blend 187](#_bookmark6)
  6. [Aviation Gasoline 187](#_bookmark7)
  7. [Aviation Turbine Fuel 187](#_bookmark8)
  8. [Biodiesel 187](#_bookmark9)
  9. [Biodiesel Blend 187](#_bookmark10)
  10. [Butanol 187](#_bookmark11)
  11. [Cetane Number 187](#_bookmark12)
  12. [Compressed Natural Gas (CNG) 188](#_bookmark0)
  13. [Denatured Fuel Ethanol 188](#_bookmark14)
  14. [Diesel Exhaust Fluid (DEF) 188](#_bookmark15)
  15. [Diesel Fuel. 188](#_bookmark16)
  16. [Director 188](#_bookmark17)
  17. [Distillate 188](#_bookmark18)

[1.18. EPA 188](#_bookmark19)

* 1. [Energy Institute (EI) 188](#_bookmark20)
  2. [Engine Fuel 188](#_bookmark21)
  3. [Engine Fuels Designed for Special Use 188](#_bookmark22)
  4. [Ethanol 188](#_bookmark23)
  5. [Ethanol Flex Fuel 188](#_bookmark24)
  6. [Flexible Fuel Vehicle 188](#_bookmark25)
  7. [Fuel Additive 188](#_bookmark26)
  8. [Fuel Cell 189](#_bookmark13)
  9. [Fuel Oil 189](#_bookmark28)
  10. [Gasoline 189](#_bookmark29)
  11. [Gasoline-Oxygenate Blend 189](#_bookmark30)
  12. [Gear Oil 189](#_bookmark31)
  13. [Hydraulic Fluid 189](#_bookmark32)
  14. [Hydrogen Fuel 189](#_bookmark33)
  15. [Internal Combustion Engine 189](#_bookmark34)
  16. [International Organization for Standardization (ISO) 189](#_bookmark35)
  17. [Kerosene. 189](#_bookmark36)
  18. [Lead Substitute 189](#_bookmark37)
  19. [Lead Substitute Engine Fuel 189](#_bookmark38)
  20. [Liquefied Natural Gas (LNG) 189](#_bookmark39)
  21. [Liquefied Petroleum Gas (LPG**).** 190](#_bookmark27)
  22. [Low Temperature Operability 190](#_bookmark41)
  23. [Lubricant 190](#_bookmark42)
  24. [Lubricity 190](#_bookmark43)
  25. [M85 Fuel Methanol 190](#_bookmark44)
  26. [Motor Octane Number 190](#_bookmark45)
  27. [Motor Oil. 190](#_bookmark46)

[1.47. Oil. 190](#_bookmark47)

[G. Uniform Fuels and Automotive Lubricants Regulation](#_TOC_250000)

* 1. [Oxygen Content of Gasoline 190](#_bookmark48)
  2. [Oxygenate 190](#_bookmark49)
  3. [Racing Gasoline 190](#_bookmark50)
  4. [Research Octane Number 190](#_bookmark51)
  5. [SAE (SAE International) 191](#_bookmark40)
  6. [Thermal Stability 191](#_bookmark53)
  7. [Tractor Hydraulic Fluid 191](#_bookmark54)
  8. [Unleaded 191](#_bookmark55)
  9. [Wholesale Purchaser Consumer 191](#_bookmark56)

[Section 2. Standard Specifications 191](#_bookmark57)

* 1. [Gasoline and Gasoline-Oxygenate Blends 191](#_bookmark58)
     1. [Gasoline and Gasoline-Oxygenate Blends 191](#_bookmark59)
     2. [Gasoline-Ethanol Blends 191](#_bookmark60)
     3. [Minimum Antiknock Index (AKI) 191](#_bookmark61)
     4. [Minimum Motor Octane Number 192](#_bookmark52)
     5. [Lead Substitute Gasoline 192](#_bookmark62)
        1. [Documentation of Exhaust Valve Seat Protection 192](#_bookmark63)
     6. [Blending 192](#_bookmark64)
  2. [Diesel Fuel 192](#_bookmark65)
     1. [Premium Diesel Fuel. 192](#_bookmark66)
     2. [Use of Other Diesel Terminology 193](#_bookmark67)
  3. [Aviation Turbine Fuels 193](#_bookmark68)
  4. [Aviation Gasoline 194](#_bookmark69)
  5. [Fuel Oils 194](#_bookmark70)
  6. [Kerosene (Kerosine) 194](#_bookmark71)
  7. [Denatured Fuel Ethanol 194](#_bookmark72)
  8. [Liquefied Petroleum (LP) Gases 194](#_bookmark73)
  9. [Liquefied Natural Gas (LNG) Vehicle Fuel 194](#_bookmark74)
  10. [Compressed Natural Gas (CNG) 194](#_bookmark75)
  11. [Ethanol Flex Fuel 194](#_bookmark76)
  12. [M85 Fuel Methanol 194](#_bookmark77)
  13. [Racing Gasoline 194](#_bookmark78)
  14. [Engine (Motor) Oil 195](#_bookmark79)
  15. [Products for Use in Lubricating Manual Transmissions, Gears, or Axles 195](#_bookmark80)
  16. [Products for Use in Lubricating Transmissions 195](#_bookmark81)
      1. [Conformance 195](#_bookmark82)
      2. [Transmission Fluid Additives 195](#_bookmark83)
  17. [Biodiesel Blendstock 196](#_bookmark85)
  18. [Butanol for Blending with Gasoline 196](#_bookmark86)
  19. [Dimethyl Ether for Fuel Purposes 196](#_bookmark87)
  20. [Hydrogen Fuel 196](#_bookmark88)
  21. [Diesel Exhaust Fluid (DEF). 196](#_bookmark89)
  22. [Products for Use in Lubricating Tractors 196](#_bookmark90)
      1. [Conformance 196](#_bookmark91)
      2. [Tractor Hydraulic Fluid Additives 196](#_bookmark92)

[Section 3. Classification and Labeling for Sale 197](#_bookmark84)

* 1. [General Considerations 197](#_bookmark84)
     1. [Documentation 197](#_bookmark93)
     2. [Retail Dispenser Labeling 197](#_bookmark94)
     3. [Grade Name. 197](#_bookmark95)
     4. [Nozzle Requirements for Automotive Gasoline, Gasoline-Oxygenate Blends, 197](#_bookmark96)
  2. [Automotive Gasoline and Automotive Gasoline-Oxygenate Blends (Including Racing Gasoline). 197](#_bookmark97)
     1. [Posting of Antiknock Index Required 197](#_bookmark98)
     2. [Use of Lead Substitute Must be Disclosed. 197](#_bookmark99)
     3. [Prohibition of Terms 197](#_bookmark100)
     4. [Method of Retail Sale. 198](#_bookmark102)
     5. [Documentation for Dispenser Labeling Purposes 198](#_bookmark103)
     6. [EPA Labeling Requirements 198](#_bookmark104)
  3. [Diesel Fuel. 199](#_bookmark101)
     1. [Labeling of Grade Required. 199](#_bookmark106)
     2. [Automotive Fuel Rating 199](#_bookmark107)
     3. [Delivery Documentation for Premium Diesel. 199](#_bookmark108)
  4. [Aviation Turbine Fuels 199](#_bookmark109)
     1. [Labeling of Grade Required 199](#_bookmark110)
     2. [NFPA Labeling Requirements Also Apply 199](#_bookmark111)
  5. [Aviation Gasoline 199](#_bookmark112)
     1. [Labeling of Grade Required 199](#_bookmark113)
     2. [NFPA Labeling Requirements Also Apply 199](#_bookmark114)
  6. [Fuel Oils 199](#_bookmark115)
     1. [Labeling of Grade Required 199](#_bookmark116)
     2. [Retail Fuel Oil. 200](#_bookmark105)
  7. [Kerosene (Kerosine) 200](#_bookmark118)
     1. [Labeling of Grade Required. 200](#_bookmark119)
     2. [Additional Labeling Requirements 200](#_bookmark120)
  8. [Ethanol Flex Fuel 200](#_bookmark121)
     1. [How to Identify Ethanol Flex Fuel 200](#_bookmark122)
     2. [FTC Labeling Requirements 200](#_bookmark123)
  9. [M85 Fuel Methanol 200](#_bookmark124)
     1. [How to Identify M85 Fuel Methanol 200](#_bookmark125)
     2. [Retail Dispenser Labeling 200](#_bookmark126)
  10. [Liquefied Petroleum Gas (LPG) 201](#_bookmark117)
      1. [How LPG is to be Identified. 201](#_bookmark117)
      2. [Retail Dispenser Labeling 201](#_bookmark128)
      3. [Additional Labeling Requirements 201](#_bookmark129)
      4. [NFPA Labeling Requirements Also Apply 201](#_bookmark130)
  11. [Compressed Natural Gas (CNG) 201](#_bookmark131)
      1. [How Compressed Natural Gas is to be Identified. 201](#_bookmark132)
      2. [Retail Sales of Compressed Natural Gas Sold as a Vehicle Fuel 201](#_bookmark133)
         1. [Retail Dispenser Labeling 201](#_bookmark134)
         2. [Nozzle Requirements for CNG 201](#_bookmark135)
  12. [Liquefied Natural Gas (LNG) 201](#_bookmark136)
      1. [How Liquefied Natural Gas is to be Identified. 201](#_bookmark137)
      2. [Labeling of Retail Dispensers of Liquefied Natural Gas Sold as a Vehicle Fuel 201](#_bookmark138)
         1. [Identification of Product 201](#_bookmark139)
         2. [Automotive Fuel Rating 201](#_bookmark140)
         3. [NFPA Labeling 201](#_bookmark141)

[3.13. Oil. 201](#_bookmark142)

* + 1. [Labeling of Vehicle Engine (Motor) Oil Required 201](#_bookmark143)
       1. [Viscosity 202](#_bookmark127)
       2. [Brand. 202](#_bookmark144)
       3. [Engine Service Category 202](#_bookmark145)
       4. [Tank Trucks or Rail Cars 202](#_bookmark146)
       5. [Documentation 203](#_bookmark147)
    2. [Labeling of Recreational Motor Oil 203](#_bookmark148)
       1. [Viscosity 203](#_bookmark149)
       2. [Intended Use. 203](#_bookmark150)
    3. [Labeling of Gear Oil 203](#_bookmark151)
       1. [Viscosity 203](#_bookmark152)

G. Uniform Fuels and Automotive Lubricants Regulation

* + - 1. [Service Category 203](#_bookmark153)
  1. [Transmission Fluid 203](#_bookmark154)
     1. [Labeling and Identification of Transmission Fluid 203](#_bookmark155)
        1. [Container Labeling 203](#_bookmark156)
        2. [Identification on Documentation 204](#_bookmark157)
        3. [Identification on Service Provider Documentation 204](#_bookmark158)
        4. [Bulk Delivery 204](#_bookmark159)
        5. [Storage Tank Labeling 204](#_bookmark160)
        6. [Documentation of Claims Made Upon Product Label 205](#_bookmark161)
  2. [Biodiesel and Biodiesel Blends 205](#_bookmark162)
     1. [Identification of Product 205](#_bookmark163)
     2. [Labeling of Retail Dispensers 205](#_bookmark164)
        1. [Labeling of Grade Required. 205](#_bookmark165)
        2. [Automotive Fuel Rating 205](#_bookmark166)
        3. [Biodiesel Blends 205](#_bookmark167)
     3. [Documentation for Dispenser Labeling Purposes 205](#_bookmark168)
     4. [Exemption 205](#_bookmark169)
  3. [Diesel Exhaust Fluid (DEF) 206](#_bookmark170)
     1. [Labeling of Diesel Exhaust Fluid (DEF) 206](#_bookmark171)
        1. [Retail Dispenser Labeling 206](#_bookmark172)
        2. [Documentation for Retailers of Bulk Product. 206](#_bookmark173)
        3. [Labeling Packaged Product 206](#_bookmark174)
        4. [Documentation for Bulk Deliveries 206](#_bookmark175)
  4. [Tractor Hydraulic Fluid 206](#_bookmark176)
     1. [Labeling and Identification of Tractor Hydraulic Fluid 206](#_bookmark177)
        1. [Container Labeling 206](#_bookmark178)
        2. [Identification on Documentation 207](#_bookmark179)
        3. [Identification on Service Provider Documentation 207](#_bookmark180)
        4. [Bulk Delivery 208](#_bookmark181)
        5. [Storage Tank Labeling 208](#_bookmark182)
        6. [Documentation of Claims Made Upon Product Label 208](#_bookmark183)

[Section 4. Retail Storage Tanks and Dispenser Filters 208](#_bookmark184)

* 1. [Water in Gasoline-Alcohol Blends, Biodiesel Blends, Ethanol Flex Fuel, Aviation Gasoline, and Aviation Turbine Fuel 208](#_bookmark185)
  2. [Water in Gasoline, Diesel, Gasoline-Ether, and Other Fuels 208](#_bookmark186)
  3. [Dispenser Filters 208](#_bookmark187)
     1. [Engine Fuel Dispensers 208](#_bookmark188)
     2. [Delivery of Aviation Fuel and Gasoline 209](#_bookmark190)
  4. [Product Storage Identification 209](#_bookmark191)
     1. [Fill Connection Labeling 209](#_bookmark192)
     2. [Declaration of Meaning of Color Code 209](#_bookmark193)
  5. [Volume of Product Information. 209](#_bookmark194)

[Section 5. Condemned Product 209](#_bookmark195)

* 1. [Stop-Sale Order at Retail 209](#_bookmark196)
  2. [Stop-Sale Order at Terminal or Bulk Plant Facility 209](#_bookmark197)

[Section 6. Product Registration 210](#_bookmark189)

* 1. [Engine Fuels Designed for Special Use 210](#_bookmark189)
     1. [Identity 210](#_bookmark199)
     2. [Address. 210](#_bookmark200)
     3. [Business Type 210](#_bookmark201)
     4. [Signature 210](#_bookmark202)

G. Uniform Fuels and Automotive Lubricants Regulation

* + 1. [Product Description 210](#_bookmark203)
    2. [Product Specification 210](#_bookmark204)
  1. [Renewal 210](#_bookmark205)
  2. [Re-registration 210](#_bookmark206)
  3. [Authority to Deny Registration. 210](#_bookmark207)
  4. [Transferability 210](#_bookmark208)

[Section 7. Test Methods and Reproducibility Limits 210](#_bookmark209)

* 1. [ASTM Standard Test Methods 210](#_bookmark210)
     1. [Premium Diesel 210](#_bookmark211)
  2. [Reproducibility Limits 211](#_bookmark198)
     1. [AKI Limits 211](#_bookmark198)
     2. [Reproducibility 211](#_bookmark212)
     3. [SAE Viscosity Grades for Engine Oils 211](#_bookmark213)
     4. [Dispute Resolution 211](#_bookmark214)
     5. [Additional Enforcement Action 211](#_bookmark215)

G. Uniform Fuels and Automotive Lubricants Regulation

THIS PAGE INTENTIONALLY LEFT BLANK

G. Uniform Fuels and Automotive Lubricants Regulation

**G. Uniform Fuels and Automotive Lubricants Regulation**

# Section 1. Definitions

* 1. **ASTM (ASTM International).** ([**www.astm.org**](http://www.astm.org/)) – The international voluntary consensus standards organiza- tion formed for the development of standards on characteristics and performance of materials, products, systems, and services, and the promotion of related knowledge.
  2. **Antiknock Index (AKI**)**.** – The arithmetic average of the Research Octane Number (RON) and Motor Octane Number (MON): AKI = (RON+MON)/2. This value is called by a variety of names, in addition to antiknock index, including: octane rating, posted octane, (R+M)/2 octane.
  3. **Automatic Transmission Fluid.** – A product intended for use in a passenger vehicle, other than a bus, as either lubricant, coolant, or liquid medium in any type of fluid automatic transmission that contains a torque con- verter. For the purposes of this regulation, fluids intended for use in continuously variable transmissions are not considered “Automatic Transmission Fluid.”

(Added 2004)

* 1. **Automotive Fuel Rating.** – The automotive fuel rating required under the amended Automotive Fuel Ratings, Certification and Posting Rule (or as amended, the Fuel Rating Rule), 16 CFR 306. Under this Rule, sellers of liquid automotive fuels, including alternative fuels, must determine, certify, and post an appropriate automotive fuel rating. The automotive fuel rating for gasoline and gasoline-oxygenate blends is the antiknock index (octane rating). The automotive fuel rating for alternative liquid automotive fuels consists of the common name of the fuel, along with a disclosure of the amount, expressed as a minimum volume percent of the principal component of the fuel. For alter- native liquid automotive fuels, a disclosure of other components, expressed as a minimum volume percent, may be included, if desired.

(Amended 2018)

* 1. **Automotive Gasoline, Automotive Gasoline-Oxygenate Blend.** – A type of fuel suitable for use in spark ignition automobile engines containing small amounts of fuel additives and also commonly used in marine and non- automotive applications.

(Amended 2018)

* 1. **Aviation Gasoline.** – A type of gasoline suitable for use as a fuel in an aviation spark-ignition internal com- bustion engine.
  2. **Aviation Turbine Fuel.** – A refined middle distillate suitable for use as a fuel in an aviation gas turbine internal combustion engine.
  3. **Biodiesel.** – A fuel comprised of at least 99 % by volume mono-alkyl esters of long chain fatty acids derived from vegetable oils or animal fats, designated B100 or B99.

(Amended 2018)

* 1. **Biodiesel Blend.** – A fuel comprised of a blend of biodiesel with hydrocarbon diesel fuel. (Amended 2018)
  2. **Butanol.** – Butyl alcohol, the chemical compound C4H9OH, a colorless substance existing in four isomeric forms.

(Added 2018)

* 1. **Cetane Number.** – A numerical measure of the ignition performance of a diesel fuel obtained by comparing it to reference fuels in a standardized engine test.

G. Uniform Fuels and Automotive Lubricants Regulation

* 1. **Compressed Natural Gas (CNG).** – Natural gas which has been compressed and dispensed into fuel storage containers and is suitable for use as an engine fuel.
  2. **Denatured Fuel Ethanol.** – An ethanol blend component for use in gasoline-ethanol blends and ethanol flex fuel. The ethanol is rendered unfit for beverage use by the addition of denaturants under formulas approved by the Alcohol and Tobacco Tax and Trade Bureau (TTB) ([**www.ttb.gov**](http://www.ttb.gov/)), by the latest version of ASTM D4806, “Standard Specification for Denatured Fuel Ethanol for Blending with Gasolines for Use as Automotive Spark Ignition Engine Fuel” describes the acceptable denaturants for denatured fuel ethanol to be blended into spark ignition engine fuels.

(Amended 2014)

* 1. **Diesel Exhaust Fluid (DEF).** – A preparation of aqueous urea [(NH2)2CO], containing 32.5 % by mass of technically-pure urea in high-purity water with quality characteristics defined by the latest version of ISO 22241, “Diesel engines – NOx reduction agent AUS 32.”

(Added 2014)

* 1. **Diesel Fuel.** – A refined hydrocarbon suitable for use as a fuel in a compression-ignition (diesel) internal com- bustion engine that may contain a combination of biodiesel, renewable diesel, and fuel additives.

(Amended 2018)

* 1. **Director. –** The Director, Commissioner, or other authority having jurisdiction over a department and/or their designated agent(s).

(Added 2018)

* 1. **Distillate.** – Any product obtained by condensing the vapors given off by boiling petroleum or its products.
  2. **EPA** ([**www.epa.gov**](http://www.epa.gov/)) – The United States Environmental Protection Agency.
  3. **Energy Institute (EI) (**[**knowledge.energyinst.org**](https://knowledge.energyinst.org/)**).** – A professional organization for the energy industry, developing standards, and other technical documents.

(Added 2018)

* 1. **Engine Fuel.** – Any liquid or gaseous matter used for the generation of power in an internal combustion engine.
  2. **Engine Fuels Designed for Special Use.** – Engine fuels designated by the Director as requiring registration. These fuels normally do not have ASTM or other national consensus standards applying to their quality or usability; common special fuels are racing fuels and those intended for agricultural and other off-road applications.
  3. **Ethanol.** – Also known as “ethyl alcohol.” Ethanol is provided in gasoline-ethanol blends by blending dena- tured fuel ethanol. (See Section 1.13. Denatured Fuel Ethanol.)

(Amended 2014)

* 1. **Ethanol Flex Fuel.** – Blends of ethanol and hydrocarbons restricted for use as fuel in ground vehicles equipped with flexible-fuel spark-ignition engines.

(Amended 2014)

* 1. **Flexible Fuel Vehicle.** – A vehicle designed to operate on either unleaded gasoline or ethanol flex fuel or mixtures of both. Flexible fuel vehicles may also be designated to run on M85 Fuel Methanol.

(Added 2018)

* 1. **Fuel Additive.** – A material added to a fuel in small amounts to impart or enhance desirable properties or to suppress undesirable properties.

(Added 2018)

G. Uniform Fuels and Automotive Lubricants Regulation

* 1. **Fuel Cell.** – An electrochemical energy conversion device in which fuel and an oxidant react to generate elec- tricity without consumption, physically or chemically, of its electrodes or electrolytes.

(Added 2012)

* 1. **Fuel Oil.** – Refined oil middle distillates, heavy distillates, or residues of refining, or blends of these, suitable for use as a fuel for heating or power generation.

(Amended 2018)

* 1. **Gasoline.** – A volatile mixture of liquid hydrocarbons containing small amounts of additives suitable for use as a fuel in a spark-ignition internal combustion engine.

(Amended 2018)

* 1. **Gasoline-Oxygenate Blend.** – A fuel consisting primarily of gasoline along with a substantial amount (more than 1 % by volume oxygenate, or more than 0.3 % by volume methanol not to exceed the total oxygen content per- mitted by applicable laws and regulations. Examples of oxygenates used in gasoline-alcohol blends are ethanol and butanol.

(Amended 2018)

* 1. **Gear Oil.** – An oil used to lubricate gears, axles, or some manual transmissions. (Added 2004)
  2. **Hydraulic Fluid.** – A product intended for use in multiple applications with a dedicated hydraulic system and sump. Such fluids cannot be used in tractors. See Tractor Hydraulic Fluid for reference.

(Added 2019)

* 1. **Hydrogen Fuel.** – A fuel composed of molecular hydrogen intended for consumption in a surface vehicle or electricity production device with an internal combustion engine or fuel cell.

(Added 2012)

* 1. **Internal Combustion Engine.** – A device used to generate power by converting chemical energy bound in the fuel via spark-ignition or compression ignition combustion into mechanical work to power a vehicle or other device.

(Added 2012)

* 1. **International Organization for Standardization (ISO) (**[**www.iso.org**](http://www.iso.org/)**).** – An independent international or- ganization with a membership of national standards and bodies.

(Added 2018)

* 1. **Kerosene.** – (or “Kerosine”) A refined middle distillate suitable for use as a fuel for heating or illuminating. (Amended 2018)
  2. **Lead Substitute.** – An EPA-registered gasoline additive suitable, when added in small amounts to fuel, to reduce or prevent exhaust valve recession (or seat wear) in automotive spark-ignition internal combustion engines designed to operate on leaded fuel.
  3. **Lead Substitute Engine Fuel.** – For labeling purposes, a gasoline or gasoline-oxygenate blend that contains a “lead substitute”.
  4. **Liquefied Natural Gas (LNG).** – Natural gas that has been liquefied at – 162 °C (– 260 °F) and stored in insulated cryogenic tanks for use as an engine fuel.

(Amended 2016)

G. Uniform Fuels and Automotive Lubricants Regulation

* 1. **Liquefied Petroleum Gas (LPG).** – A mixture of normally gaseous hydrocarbons, predominantly propane, or butane, or both, that has been liquefied by compression or cooling, or both to facilitate storage, transport, and handling.
  2. **Low Temperature Operability.** – A condition which allows the uninterrupted operation of a diesel engine through the continuous flow of fuel throughout its fuel delivery system at low temperatures. Fuels with adequate low temperature operability characteristics have the ability to avoid wax precipitation and clogging in fuel filters.

(Added 1998) (Amended 1999)

* 1. **Lubricant.** – Oil. (See 1.46. Oil below.). (Added 2008)
  2. **Lubricity**. – A qualitative term describing the ability of a fluid to affect friction between, and wear to, surfaces in relative motion under load.

(Added 2003)

* 1. **M85 Fuel Methanol.** – A blend of methanol and hydrocarbons of which the methanol portion is nominally 70 to 85 volume percent.
  2. **Motor Octane Number.** – A numerical indication of a spark-ignition engine fuel’s resistance to knock obtained by comparison with reference fuels in a standardized ASTM D2700, “Standard Test Method for Motor Octane Num- ber of Spark-Ignition Engine Fuel.
  3. **Motor Oil.** – An oil that reduces friction and wear between the moving parts within a reciprocating internal combustion engine and also serves as a coolant. For the purposes of this regulation, “vehicle motor oil” refers to motor oil which is intended for use in light- to heavy-duty vehicles including cars, sport utility vehicles, vans, trucks, buses, and off-road farming and construction equipment. For the purposes of this regulation, “recreational motor oil” refers to motor oil which is intended for use in four-stroke cycle engines used in motorcycles, ATVs, and lawn and garden equipment. For the purposes of this regulation, motor oil also means engine oil.

(Added 2004)

* 1. **MTBE.** – Methyl tertiary-butyl ether, the chemical compound (CH3)3COCH3 [C5H12O]. (Added 2008) (Amended 2018)
  2. **Oil.** – A motor oil, engine oil, and/or gear oil. (Added 2004)
  3. **Oxygen Content of Gasoline.** – The percentage of oxygen contained in a gasoline. (Amended 2018)
  4. **Oxygenate.** – An oxygen-containing, ashless, organic compound, such as an alcohol or ether, which can be used as a fuel or fuel supplement.
  5. **Racing Gasoline.** – A specialty fuel typically used in non-road racing vehicles that is generally of lower vola- tility, has a narrower boiling range and a higher octane rating than gasolines made for use in conventional passenger vehicles.

(Added 2018)

* 1. **Research Octane Number.** – A numerical indication of a spark-ignition engine fuel’s resistance to knock obtained by comparison with reference fuels in a standardized in the latest version of ASTM D2699, “Standard Test Method for Research Octane Number of Spark-Ignition Engine Fuel.”

(Amended 2018)

G. Uniform Fuels and Automotive Lubricants Regulation

* 1. **SAE (SAE International) (**[**www.sae.org**](http://www.sae.org/)**).** – A technical organization for engineers, scientists, technicians, and others who cooperate closely in the engineering, design, manufacture, use, and maintainability of self-propelled vehicles.
  2. **Thermal Stability.** – The ability of a fuel to resist the thermal stress which is experienced by the fuel when exposed to high temperatures in a fuel delivery system. Such stress can lead to formation of insoluble gums or organic particulates. Insolubles (e.g., gums or organic particulates) can clog fuel filters and contribute to injector deposits.

(Added 1998) (Amended 1999 and 2018)

* 1. **Tractor Hydraulic Fluid.** – A product intended for use in tractors with a common sump for the transmission, final drives, wet brakes, axles, and hydraulic system.

(Added 2019)

* 1. **Unleaded.** – When used in conjunction with “engine fuel” or “gasoline” means any gasoline or gasoline-oxy- genate blend to which no lead or phosphorus compounds have been intentionally added and which contains not more than 0.013 g of lead per liter (0.05 g lead per U.S. gallon) and not more than 0.0013 g of phosphorus per liter (0.005 g phosphorus per U.S. gallon).
  2. **Wholesale Purchaser Consumer.** – Any person who is an ultimate consumer of gasoline, fuel methanol, eth- anol flex fuel, diesel fuel, biodiesel, biodiesel blends, fuel oil, kerosene, aviation turbine fuels, natural gas, compressed natural gas, or liquefied petroleum gas and who purchases or obtains the product from a supplier and receives delivery of that product into a storage tank.

(Added 1998) (Amended 1999 and 2014)

# Section 2. Standard Specifications

## Gasoline and Gasoline-Oxygenate Blends.

* + 1. **Gasoline and Gasoline-Oxygenate Blends** (as defined in this regulation)**.** – Shall meet the latest version of ASTM D4814, “Standard Specification for Automotive Spark-Ignition Engine Fuel” except for the permissible offsets for ethanol blends as provided in Section 2.1.2. Gasoline-Ethanol Blends.
       1. The maximum concentration of oxygenates contained in gasoline-oxygenate blends shall not exceed those permitted by the EPA under Section 211 of the Clean Air Act and applicable waivers.

(Added 2009) (Amended 2018)

* + 1. **Gasoline-Ethanol Blends. –** When gasoline is blended with denatured fuel ethanol, the denatured fuel ethanol shall meet the latest version of ASTM D4806, “Standard Specification for Denatured Fuel Ethanol for Blending with Gasolines for Use as Automotive Spark-Ignition Engine Fuel,” and the blend shall meet the latest version of ASTM D4814, “Standard Specification for Automotive Spark-Ignition Engine Fuel,” with the follow- ing permissible exceptions:
       1. The maximum vapor pressure shall not exceed the latest version of ASTM D4814, “Standard Specifica- tion for Automotive Spark-Ignition Engine Fuel,” limits by more than 1.0 psi for blends from June 1 through September 15 as allowed by EPA per 40 CFR 80.27(d).

(Amended 2016, 2018, and 2019)

***NOTE:*** *The values shown above appear only in U.S. customary units to ensure that the values are identical to those in ASTM standards and the Environmental Protection Agency regulation.*

(Added 2009) (Amended 2012 and 2016)

* + 1. **Minimum Antiknock Index (AKI).** – The AKI shall not be less than the AKI posted on the product dispenser or as certified on the invoice, bill of lading, shipping paper, or other documentation;

G. Uniform Fuels and Automotive Lubricants Regulation

* + 1. **Minimum Motor Octane Number.** – The minimum motor octane number shall not be less than 82 for gasoline with an AKI of 87 or greater;
    2. **Lead Substitute Gasoline.** – Gasoline and gasoline-oxygenate blends sold as “lead substitute” gasoline shall contain a lead substitute which provides protection against exhaust valve seat recession equivalent to at least

0.026 g of lead per liter (0.10 g per U.S. gallon).

* + - 1. **Documentation of Exhaust Valve Seat Protection.** – Upon the request of the Director, the lead substitute additive manufacturer shall provide documentation to the Director that demonstrates that the treat- ment level recommended by the additive manufacturer provides protection against exhaust valve seat reces- sion equivalent to or better than 0.026 g/L (0.1 g/gal) lead. The Director may review the documentation and approve the lead substitute additive before such additive is blended into gasoline. This documentation shall consist of:
         1. test results as published in the Federal Register by the EPA Administrator as required in Sec- tion 211(f)(2) of the Clean Air Act; or
         2. until such time as the EPA Administrator develops and publishes a test procedure to determine the additive’s effectiveness in reducing valve seat wear, test results and description of the test proce- dures used in comparing the effectiveness of 0.026 g per liter lead and the recommended treatment level of the lead substitute additive shall be provided.
    1. **Blending.** – Leaded, lead substitute, and unleaded gasoline-oxygenate blends shall be blended according to the EPA “substantially similar” rule or an EPA waiver for unleaded fuel.

(Amended 2009)

* 1. **Diesel Fuel.** – Shall meet the following requirements, based on the biodiesel concentration of the fuel:

1. Diesel fuel that contains less than or equal to 5 % by volume biodiesel shall meet the latest version of ASTM D975, “Standard Specifications for Diesel Fuels” and shall be sold as diesel fuel.
2. Diesel fuel that contains greater than or equal to 6 % by volume biodiesel and that contains less than or equal to 20 % by volume shall meet the latest version of ASTM D7467, “Standard Specifications for Diesel Fuel Oil, Biodiesel Blend (B6 to B20).”
3. Only fuel additive registered with the U.S. EPA may be used to additize diesel fuel, and the final product shall meet the latest version of ASTM D975 and/or ASTM D7467.

(Amended 2003 and 2018)

* + 1. **Premium Diesel Fuel.** – All diesel fuels identified on retail dispensers as premium, super, supreme, or premier must conform to the following minimum requirements:
       1. **Cetane Number.** – A minimum cetane number of 47.0 as determined by the latest version of ASTM D613, “Standard Test Method for Cetane Number of Diesel Fuel Oil.”

***NOTE:*** ASTM D613, “Standard Test Method for Cetane Number of Diesel Fuel Oil” is the referee method; however, the following methods can be used to determine cetane number: the latest version of ASTM D6890, “Standard Test Method for Determination of Ignition Delay and Derived Cetane Num- ber” (DCN) of Diesel Fuel Oils by Combustion in a Constant Volume Chamber”; and ASTM D7668, “Standard Test Method for Determination of Derived Cetane Number (DCN) of Diesel Fuel Oils—Ig- nition Delay and Combustion Delay Using a Constant Volume Combustion Chamber Method.”

(Note added 2019)

* + - 1. **Low Temperature Operability.** – A cold flow performance measurement which meets the latest ver- sion of ASTM D975, “Standard Specification for Diesel Fuel,” tenth percentile minimum ambient air

G. Uniform Fuels and Automotive Lubricants Regulation

temperature charts and maps by the latest version of either ASTM D2500, “Standard Test Method for Cloud Point of Petroleum Products and Liquid Fuels” or ASTM D4539, “Standard Test Method for Filterability of Diesel Fuels by Low Temperature Flow Test, (LTFT).” The latest version of ASTM D6371, “Standard Test Method for Cold Filter Plugging Point of Diesel and Heating Fuels” may be used when the test results are a maximum of 6 °C below the Cloud Point. Low temperature operability is only applicable October 1 to March 31 of each year.

* + - 1. **Lubricity.** – A maximum wear scar diameter of 460 micrometers as determined by the latest version ASTM D6079, “Standard Test Method for Evaluating Lubricity of Diesel Fuels by the High-Frequency Reciprocating Rig (HFRR).”

***NOTE:*** The latest version of ASTM D6079, “Standard Test Method for Evaluating Lubricity of Diesel Fuels by the High-Frequency Reciprocating Rig (HFRR)” is the referee method; however, the latest version of ASTM D7688, “Standard Test Method for Evaluating Lubricity of Diesel Fuels by the High- Frequency Reciprocating Rig (HFRR) by Visual Observation” can be used.

(Note added 2019)

* + - 1. **Corrosion.** – A minimum rating of B+ as determined by the latest version of NACE TM0172, “Deter- mining Corrosive Properties of Cargoes in Petroleum Product Pipelines.”

***NOTE:*** The latest version of NACE TM0172 “Determining Corrosive Properties of Cargoes in Petro- leum Product Pipelines” is the referee method. The latest version of ASTM D7548 “Standard Test Method for Determination of Accelerated Iron Corrosion in Petroleum Products” can be used.

(Added 2019)

* + - 1. **Filter Blocking Tendency (FBT).** – A maximum of 2.2 by the latest version of ASTM D2068, “Standard Test Method for Determining Filter Blocking Tendency”, following procedure B.

(Added 2019)

* + - 1. **Injector Deposit Control.** – Maximum power loss in keep-clean mode of 2 % by the latest version of Coordinating European Council, CEC F-98-08, “Direct Injection, Common Rail Diesel Engine Nozzle Coking Test.”

(Added 2019)

* + 1. **Use of Other Diesel Terminology.** – For any terms other than premium, super, supreme, or premier included in the diesel fuel product or grade name and/or advertisements and claims displayed on dispensers, pump toppers, pole signs and bollard signs which imply improved performance, the product must have a clearly-defined fuel property with a substantiated functional benefit. Such property must be measurable utilizing industry ac- cepted test methodologies developed by recognized standards organizations such as ASTM, SAE, and CEC to allow verification of the improved performance.

(Added 2019)

(Amended 2003 and 2019)

* 1. **Aviation Turbine Fuels.** – Shall meet the latest version of the following standards as appropriate:

1. ASTM D1655, “Standard Specification for Aviation Turbine Fuels.”
2. ASTM D6615, “Standard Specification for Jet B Wide-Cut Aviation Turbine Fuel.”
3. ASTM D7223, “Standard Specification for Aviation Certification Turbine Fuel.”
4. ASTM D7566, “Standard Specification for Aviation Turbine Fuel Containing Synthesized Hydrocarbons.” (Amended 2018)

G. Uniform Fuels and Automotive Lubricants Regulation

* 1. **Aviation Gasoline.** – Shall meet the latest version of one of the following as appropriate:

1. ASTM D910, “Standard Specification Leaded for Aviation Gasolines.”
2. ASTM D6227, “Standard Specification for Unleaded Aviation Gasoline Containing a Non-hydrocarbon Component.”
3. ASTM 7547, “Standard Specification for Hydrocarbon Unleaded Aviation Gasoline.” (Amended 2008 and 2018)
   1. **Fuel Oils.** – Shall meet the latest version of ASTM D396, “Standard Specification for Fuel Oils.”
   2. **Kerosene (Kerosine).** – Shall meet the latest version of ASTM D3699, “Standard Specification for Kerosine.”
   3. **Denatured Fuel Ethanol.** – Intended for blending with gasoline shall meet the latest version of ASTM D4806, “Standard Specification for Denatured Fuel Ethanol for Blending with Gasolines for Use as Automotive Spark-Igni- tion Engine Fuel.”

(Amended 2014)

* 1. **Liquefied Petroleum (LP) Gases.** – Shall meet the latest version ASTM D1835, “Standard Specification for Liquefied Petroleum (LP) Gases.”

***NOTE:*** *Also reference Gas Processors Association 2140, Liquefied Petroleum Gas Specification and Test Methods.*

* 1. **Liquefied Natural Gas (LNG) Vehicle Fuel.** – Shall meet the latest version of SAE J2699, “Liquefied Natural Gas (LNG) Vehicle Fuel.”

(Added 2018)

* 1. **Compressed Natural Gas (CNG).** – Shall meet the latest version of SAE J1616, “Recommended Practice for Compressed Natural Gas Vehicle Fuel.”
  2. **Ethanol Flex Fuel.** – Ethanol flex fuel is covered by one of two ASTM standards based on the ethanol con- centration of blend:

1. Ethanol flex fuel containing 51 to 83 volume percent ethanol shall meet the latest version of ASTM D5798, “Standard Specification for Ethanol Fuel Blends for Flexible Fuel Automotive Spark-Ignition Engines”; and
2. Ethanol flex fuel containing 16 to 50 volume percent ethanol shall be blended, stored, delivered and offered for consumption in accordance with the latest version of ASTM D7794, “Standard Practice for Blending Mid-Level Ethanol Fuel Blends for Flexible Fuel Vehicles with Automotive Spark-Ignition Engines.”

(Amended 2018)

(Added 1997) (Amended 2014 and 2018)

* 1. **M85 Fuel Methanol.** – Shall meet the latest version of ASTM D5797, “Standard Specification for Methanol Fuel Blends (M51-M85) for Methanol-Capable Automotive Spark Ignition Engines.”

(Added 1997)

* 1. **Racing Gasoline.** – Shall meet the following requirements:

1. the Minimum Antiknock Index (AKI) shall not be less than the AKI posted on the product dispenser or as certified on the invoice, bill of lading, shipping paper, or other documentation.

G. Uniform Fuels and Automotive Lubricants Regulation

1. the product specification limits shall be those as declared by the manufacturer’s product specifications. Upon the request of the Director, each supplier of racing gasoline shall provide a copy of the manufacturer’s product specifications.

(Added 2018)

* 1. **Engine (Motor) Oil.** – Shall not be sold or distributed for use unless the product conforms to the following specifications:

1. performance claims listed on the label shall be evaluated against the latest version of SAE J183, “Engine Oil Performance and Engine Service Classification,” API 1509 “Engine Oil Licensing and Certification System,” European Automobile Manufacturers’ Association (ACEA), “European Oil Sequences,” or other “Vehicle or Engine Manufacturer Standards” as applicable; and
2. the product shall meet its labeled viscosity grade specification as specified in the latest version of SAE J300, “Engine Oil Viscosity Classification.”

(Added 2004) (Amended 2014)

* 1. **Products for Use in Lubricating Manual Transmissions, Gears, or Axles.** – Shall not be sold or distributed for use in lubricating manual transmissions, gears, or axles unless the product conforms to the following specifications:

1. it is labeled with one or more of the service designations found in the latest version of the SAE Information Report on axle and manual transmission lubricants, SAE J308, and API Publication 1560, and meets all ap- plicable requirements of those designations;
2. the product shall meet its labeled viscosity grade classification as specified in the latest version of SAE J306; and
3. the product shall be free from water and suspended matter when tested by means of centrifuge, in accordance with the latest version of ASTM D2273, “Standard Test Method for Trace Sediment in Lubricating Oils.”

(Added 2004)

* 1. **Products for Use in Lubricating Transmissions.** – Transmission fluids shall meet the original equipment manufacturer’s requirements for those transmissions or have demonstrated performance claims to be suitable for use in those transmissions. Where a fluid can be licensed against an original equipment manufacturer’s specification, evidence of current licensing by the marketer is acceptable documentation of performance against the specification. In the absence of a license from the original equipment manufacturer, adherence to the original equipment manufac- turer’s recommended requirements shall be assessed after testing per relevant methods available to the lubricants industry and the state regulatory agency. Suitability for use claims shall be based upon appropriate field, bench, and/or transmission rig testing. Any manufacturer of a transmission fluid making suitable-for-use claims shall provide, upon request by a duly authorized representative of the Director, credible documentation of such claims. If the product performance claims published by a blender and/or marketer are based on the claim(s) of one or more additive suppliers, documentation of the claims may be requested in confidence by a duly authorized representative of the Director. Supporting data may be supplied directly to the Director’s office by the additive supplier(s).

(Added 2004) (Amended 2017)

* + 1. **Conformance. –** Conformance of a fluid per Section 2.14. Products for Use in Lubricating Transmis- sions does not absolve the obligations of a fluid licensee with respect to the licensing original equipment manu- facturer or the original equipment manufacturer’s licensing agent(s), where relevant.

(Added 2017)

* + 1. **Transmission Fluid Additives.** – Any material offered for sale or sold as an additive to transmission fluids shall be compatible with the transmission fluid to which it is added and shall meet all performance claims as stated on the label or published on any website referenced by the label. Any manufacturer of any such product

G. Uniform Fuels and Automotive Lubricants Regulation

sold in this state shall provide, upon request by a duly authorized representative of the Director, documentation of any claims made on their product label or published on any website referenced by the label.

(Added 2017)

* 1. **Biodiesel Blendstock.** – Biodiesel intended for blending with diesel fuel shall meet the latest version of ASTM D6751, “Standard Specification for Biodiesel Fuel Blend Stock (B100) for Middle Distillate Fuels.” Any blend stock less than 99 % by volume biodiesel (no more than 1 % by volume diesel fuel). Any blend stock less than 99 % by volume shall not be used as a commercial blend stock for biodiesel blends without the permission of the Director.

(Added 2004) (Amended 2018)

* 1. **Butanol for Blending with Gasoline.** – Shall meet the latest version of ASTM D7862, “Standard Specifica- tions for Butanol for Blending with Gasoline for Use as Automotive Spark-Ignition Engine Fuel.”

(Added 2018)

* 1. **Dimethyl Ether for Fuel Purposes.** – Shall meet the latest version of ASTM D7901, “Standard Specifications for Dimethyl Ether for Fuel Purposes.”

(Added 2018)

* 1. **Hydrogen Fuel.** – Shall meet the latest version of SAE J2719, “Hydrogen Fuel Quality for Fuel Cell Vehicles.” (Added 2012)
  2. **Diesel Exhaust Fluid (DEF). –** Shall meet the latest version of the ISO 22241, “Diesel engines – NOx reduc- tion agent AUS 32.”

(Added 2014)

* 1. **Products for Use in Lubricating Tractors.** – Tractor hydraulic fluids shall meet at least one current and/or verifiable original equipment manufacturer’s specifications for respective tractors. A specification is deemed verifi- able if all necessary bench and laboratory tests are available to verify the fluid’s ability to pass those requirements set out by the original equipment manufacturer. A list of current and verifiable specifications is located on the NCWM website (**www.ncwm.com**). Where a fluid can be licensed against an original equipment manufacturer’s specification, evidence of current licensing by the marketer is acceptable documentation of performance against the specification. In the absence of a license from the original equipment manufacturer, adherence to the original equipment manufac- turer’s specifications shall be assessed after testing per relevant methods available to the lubricants industry and the regulatory agency. Suitability for use claims shall be based upon appropriate field, bench, and/or rig testing. Any manufacturer of a tractor hydraulic fluid making suitable for use claims shall provide, upon request by a duly author- ized representative of the Director, credible documentation of such claims. If the product performance claims pub- lished by a blender and/or marketer are based on the claim(s) of one or more additive suppliers, documentation of the claims shall be provided upon request to a duly authorized representative of the Director. Supporting data shall, upon request, be supplied directly to the Director’s office by the additive supplier(s).
     1. **Conformance.** – Conformance of a fluid per Section 2.22. Products for Use in Lubricating Tractors does not absolve the obligations of a fluid licensee with respect to the licensing original equipment manufacturer or the original equipment manufacturer’s licensing agent(s), where relevant.
     2. **Tractor Hydraulic Fluid Additives.** – Any material offered for sale or sold as an additive to tractor hydraulic fluids shall be compatible with the tractor hydraulic fluid to which it is added and shall meet all perfor- mance claims as stated on the label or published on any website referenced by the label. Any manufacturer of any such product sold shall provide, upon request by a duly authorized representative of the Director, documentation of any claims made on their product label or published on any website referenced by the label.

(Added 2019)

G. Uniform Fuels and Automotive Lubricants Regulation

# Section 3. Classification and Labeling for Sale

## General Considerations.

* + 1. **Documentation.** – When products regulated by this rule are sold, an invoice, bill of lading, shipping paper, or other documentation must accompany each delivery other than a retail sale. This document must identify the quantity, the name of the product, the particular grade of the product, the applicable automotive fuel rating, and oxygenate type and content (if applicable), the name and address of the seller and buyer, and the date and time of the sale. Documentation must be retained at the retail establishment for a period not less than one year.

(Amended 2008)

* + 1. **Retail Dispenser Labeling.** – All retail dispensing devices must identify conspicuously the type of product (exception: gasoline and gasoline-oxygenate blends), the particular grade of the product (exception: No. 2 Die- sel), and the applicable automotive fuel rating.

(Amended 2018)

* + 1. **Grade Name.** – The sale of any product under any grade name that indicates to the purchaser that it is of a certain automotive fuel rating or ASTM grade shall not be permitted unless the automotive fuel rating or grade indicated in the grade name is consistent with the value and meets the requirements of Section 2, Standard Spec- ifications.
    2. **Nozzle Requirements for Automotive Gasoline, Gasoline-Oxygenate Blends, and Diesel Fuel Dis- pensers.** – Each retail dispensing device from which fuel products are sold shall be equipped with a nozzle spout having a diameter that conforms with the latest version of SAE J285, “Dispenser Nozzle Spouts for Liquid Fuel Intended for Use with Spark-Ignition and Compression Ignition Engines.”

(Added 2018)

(Amended 2018)

## Automotive Gasoline and Automotive Gasoline-Oxygenate Blends (Including Racing Gasoline).

* + 1. **Posting of Antiknock Index Required.** – Automotive gasoline and automotive gasoline-oxygenate blends shall post the minimum antiknock index in accordance with applicable regulations, 16 CFR 306 issued pursuant to the “Petroleum Marketing Practices Act,” as amended.

(Amended 2018)

* + 1. **Use of Lead Substitute Must be Disclosed.** – Each dispensing device from which gasoline or gasoline- oxygenate blends containing a lead substitute is dispensed shall display the following legend: “Contains Lead Substitute.” The lettering of this legend shall not be less than 12.7 mm (½ in) in height and the color of the lettering shall be in definite contrast to the background color to which it is applied.
    2. **Prohibition of Terms.** – It is prohibited to use specific terms to describe a grade of gasoline or gasoline- oxygenate blend unless it meets the minimum antiknock index requirement shown in Table 1. Minimum Anti- knock Index Requirements.

G. Uniform Fuels and Automotive Lubricants Regulation

|  |  |  |
| --- | --- | --- |
| **Table 1. Minimum Antiknock Index Requirements** | | |
| **Term** | **Minimum Antiknock Index** | |
| **ASTM D4814 Altitude Reduc- tion Areas IV and V** | **All Other ASTM D4814 Areas** |
| Premium, Super, Supreme, High Test | 90 | 91 |
| Midgrade, Plus | 87 | 89 |
| Regular, Unleaded (alone) | 85 | 87 |
| Economy | -- | 86 |

(Table 1. Amended 1997 and 2018)

* + 1. **Method of Retail Sale.** – Type of Oxygenate must be disclosed. All automotive gasoline or automotive gasoline-oxygenate blends, or racing gasoline kept, offered, or exposed for sale, or sold at retail containing more than one volume percent oxygenate shall be identified as “with” or “containing” (or similar wording) the predom- inant oxygenate in the engine fuel. For example, the label may read “contains ethanol” or “with methyl *tertiary*- butyl ether (MTBE).” The oxygenate contributing the largest mass percent oxygen to the blend shall be consid- ered the predominant oxygenate. Where mixtures of only ethers are present, the retailer may post the predominant oxygenate followed by the phrase “or other ethers” or alternatively post the phrase “contains MTBE or other ethers.” In addition, gasoline-methanol blends containing more than 0.3 % by volume methanol shall be identified as “with” or “containing” methanol. This information shall be posted on the upper 50 % of the dispenser front panel in a position clear and conspicuous from the driver’s position in a type at least 12.7 mm (½ in) in height,

1.5 mm (1/16 in) stroke (width of type). (Amended 1996 and 2018)

* + 1. **Documentation for Dispenser Labeling Purposes.** – For automotive gasoline, automotive gasoline-ox- ygenate blends or racing gasoline, the retailer shall be provided, at the time of delivery of the fuel, on product transfer documents such as an invoice, bill of lading, shipping paper, or other documentation:
       1. Information that complies with 40 CFR 80.1503 when the fuel contains ethanol. (Added 2014)
       2. For fuels that do not contain ethanol, information that complies with 40 CFR 80.1503 and a declaration of the predominant oxygenate or combination of oxygenates present in concentrations sufficient to yield an oxygenate content of at least 1.0 % by volume in the fuel. Where mixtures of only ethers are present, the fuel supplier may identify either the predominant oxygenate in the fuel (i.e., the oxygenate contrib- uting the largest mass percent oxygen) or alternatively, use the phrase “contains MTBE or other ethers.”

(Added 2014)

* + - 1. Gasoline containing more than 0.3 % by volume methanol shall be identified as “with” or “containing” methanol.

(Added 2014) (Amended 2018)

(Amended 1996, 2014, and 2018)

* + 1. **EPA Labeling Requirements. –** Retailers and wholesale purchaser-consumers of gasoline shall comply with the EPA pump labeling requirements for gasoline containing greater than 10 volume percent (v%) up to 15 volume percent (v%) ethanol (E15) under 40 CFR 80.1501. (For additional information, refer to Section 3.8.2. FTC Labeling Requirements.)

(Added 2012) (Amended 2018)

(Amended 2018)

G. Uniform Fuels and Automotive Lubricants Regulation

## Diesel Fuel.

* + 1. **Labeling of Grade Required.** – Diesel Fuel other than No 2-D shall be identified by grade. (Amended 2018)
    2. **Automotive Fuel Rating.** – Diesel fuel containing 6 % to 20 % by volume biodiesel shall be labeled with its automotive fuel rating in accordance with the FTC “Automotive Fuel Ratings, Certification and Posting Rule,” 16 CFR 306.

(Added 2018)

* + 1. **Delivery Documentation for Premium Diesel.** – Before or at the time of delivery of premium diesel fuel, the retailer or the wholesale purchaser-consumer shall be provided on an invoice, bill of lading, shipping paper, or other documentation a declaration of all performance properties that qualifies the fuel as premium diesel fuel as required in Section 2.2.1. Premium Diesel Fuel.

(Added 1998) (Amended 1999)

(Amended 1998, 1999, 2008, 2012, and 2018)

## Aviation Turbine Fuels.

* + 1. **Labeling of Grade Required.** – Aviation turbine fuels shall be identified by the grade terms contained in applicable ASTM Standard Specifications. (See EI 1542 for additional details.)

(Amended 2018)

* + 1. **NFPA Labeling Requirements Also Apply.** [***NOTE 1***, page 199] – Each dispenser or airport fuel truck dispens- ing aviation turbine fuels shall be labeled in accordance with the latest version of National Fire Protection Asso- ciation (NFPA 407), “Standard for Aircraft Fuel Servicing.”

***NOTE 1:*** *For example, NFPA 407, 2017 edition: Section 6.1.11.3. Signage. Each aircraft fuel servicing vehicle or cart shall have signage viewable from all sides of the vehicle. Signs shall have letters at least 75 mm (3 in) high. Signs shall be of a color contrasting sharply with the background for visibility. The words “FLAMMA- BLE,” “NO SMOKING,” and the name of the product carried, such as JET A, JET B, GASOLINE, or AVGAS shall appear on each sign. (****NOTE:*** *Refer to the latest version of NFPA 407.)*

(Amended 2018)

## Aviation Gasoline.

* + 1. **Labeling of Grade Required.** – Aviation gasoline shall be identified by the grade terms contained in the latest version of ASTM Standard Specifications. (See EI 1542, “Identification Markings for Dedicated Aviation Fuel Manufacturing and Distribution Facilities, Airport Storage and Mobile Fueling Equipment” for additional detail.)

(Amended 2008 and 2018)

* + 1. **NFPA Labeling Requirements Also Apply.** [***NOTE 1***, page 199] – Each dispenser or airport fuel truck dispens- ing aviation gasoline shall be labeled in accordance with the most recent edition of National Fire Protection As- sociation (NFPA) 407, “Standard for Aircraft Fuel Servicing.”

(Amended 2018)

## Fuel Oils.

* + 1. **Labeling of Grade Required.** – Fuel Oil shall be identified by the grades contained in the latest version of ASTM D396, “Standard Specification for Fuel Oils.”

(Amended 2018)

G. Uniform Fuels and Automotive Lubricants Regulation

* + 1. **Retail Fuel Oil.** – Dispensers shall display the following legend:

“Warning – Not Suitable for Use in Unvented Heaters Requiring No. 1-K Kerosene.”

The lettering of this legend shall not be less than 12.7 mm (1/2 in) in height by 1.5 mm (1/16 in) strokes (width of type), block style letters, and the color of lettering shall be in definite contrast to the background color to which it is applied.

(Added 2018)

(Amended 2008 and 2018)

## Kerosene (Kerosine).

* + 1. **Labeling of Grade Required.** – Kerosene shall be identified by the grades No. 1-K or No. 2-K.
    2. **Additional Labeling Requirements**. – Each retail dispenser of kerosene shall be labeled as 1-K Kerosene or 2-K. In addition, No. 2-K dispensers shall display the following legend:

“Warning – Not Suitable for Use in Unvented Heaters Requiring No. 1-K”

The lettering of this legend shall not be less than 12.7 mm (1/2 in) in height by 1.5 mm (1/16 in) stroke; block style letters and the color of lettering shall be in definite contrast to the background color to which it is applied.

## Ethanol Flex Fuel.

* + 1. **How to Identify Ethanol Flex Fuel.** – Ethanol flex fuel shall be identified as Ethanol Flex Fuel or EXX Flex Fuel.
    2. **FTC Labeling Requirements.** – Ethanol flex fuel shall be identified and labeled in accordance with the Federal Trade Commission, Automotive Fuel Ratings, Certification and Posting, 16 CFR 306, as amended. (For additional information, refer to Section 3.2.6. EPA Labeling Requirements.)

(Amended 2007, 2008, 2014, and 2018)

## M85 Fuel Methanol.

* + 1. **How to Identify M85 Fuel Methanol.** – Fuel methanol shall be identified as M85.

## Example:

M85

## Retail Dispenser Labeling.

* + - 1. Fuel methanol shall be labeled with its automotive fuel rating in accordance with 16 CFR 306.

## Example:

M85 Methanol

* + - 1. A label shall be posted which states “For Use in Vehicles Capable of Using M85 Only.” This infor- mation shall be clearly and conspicuously posted on the upper 50 % of the dispenser front panel in a type of at least 12.7 mm (1/2 in) in height, 1.5 mm (1/16 in) stroke (width of type).

(Amended 2008)

G. Uniform Fuels and Automotive Lubricants Regulation

## Liquefied Petroleum Gas (LPG).

* + 1. **How LPG is to be Identified.** – Liquefied petroleum gases shall be identified by grades Commercial Propane, Commercial Butane, Commercial PB Mixtures or Special-Duty Propane (HD5).
    2. **Retail Dispenser Labeling.** – Each retail dispenser of LPGs shall be labeled as “Commercial Propane,” “Commercial Butane,” “Commercial PB Mixtures,” or “Special-Duty Propane (HD5).”
    3. **Additional Labeling Requirements.** – LPG shall be labeled with its automotive fuel rating in accordance with 16 CFR 306.
    4. **NFPA Labeling Requirements Also Apply.** (Refer to the most recent edition of NFPA 58, “Liquified Petroleum Gas Code”)

## Compressed Natural Gas (CNG).

* + 1. **How Compressed Natural Gas is to be Identified.** – For the purposes of this regulation, compressed natural gas shall be identified by the term “Compressed Natural Gas” or “CNG.”

## Retail Sales of Compressed Natural Gas Sold as a Vehicle Fuel.

## Retail Dispenser Labeling.

* + - * 1. **Identification of Product.** – Each retail dispenser of CNG shall be labeled as “Compressed Natural Gas.”
        2. **Non-Liquid Alternative Vehicle Fuel Rating.** – CNG shall be labeled with its non-liquid alternative vehicle fuel rating in accordance with 16 CFR 309.

(Added 2018)

* + - * 1. **NFPA Labeling.** – NFPA Labeling requirements also apply. (Refer to NFPA 52, “Vehicular Natural Gas Fuel Systems Code”)
      1. **Nozzle Requirements for CNG.** – CNG fueling nozzles shall comply with ANSI/AGA/CGA NGV 1.

## Liquefied Natural Gas (LNG).

* + 1. **How Liquefied Natural Gas is to be Identified.** – For the purposes of this regulation, liquefied natural gas shall be identified by the term “Liquefied Natural Gas” or “LNG.”

## Labeling of Retail Dispensers of Liquefied Natural Gas Sold as a Vehicle Fuel.

* + - 1. **Identification of Product.** – Each retail dispenser of LNG shall be labeled as “Liquefied Natural Gas.”
      2. **Automotive Fuel Rating.** – LNG automotive fuel shall be labeled with its automotive fuel rating in accordance with 16 CFR 306.
      3. **NFPA Labeling.** – NFPA Labeling requirements also apply. (Refer to NFPA 57, “Liquefied Nat- ural Gas (LNG) Vehicular Fuel Systems Code”)

## Oil.

## Labeling of Vehicle Engine (Motor) Oil Required.

G. Uniform Fuels and Automotive Lubricants Regulation

* + - 1. **Viscosity.** – The label on any vehicle engine (motor) oil container, receptacle, dispenser, or storage tank and the invoice or receipt from service on an engine that includes the installation of bulk vehicle engine (motor) oil dispensed from a receptacle, dispenser, or storage tank shall contain the viscosity grade classifi- cation preceded by the letters “SAE” in accordance with the SAE International’s latest version of SAE J300, “Engine Oil Viscosity Classification.”

(Amended 2012 and 2014)

* + - 1. **Brand.** – The label on any vehicle engine (motor) oil container and the invoice or receipt from service on an engine that includes the installation of bulk vehicle engine (motor) oil dispensed from a recep- tacle, dispenser, or storage tank shall contain the name, brand, trademark, or trade name of the vehicle engine (motor) oil.

(Added 2012 and 2014)

* + - 1. **Engine Service Category.** – The label on any vehicle engine (motor) oil container, receptacle, dispenser or storage tank and the invoice or receipt from service on an engine that includes the installation of bulk vehicle engine (motor) oil dispensed from a receptacle, dispenser, or storage tank shall contain the engine service category, or categories, displayed in letters not less than 3.18 mm (1/8 in) in height, as defined by the latest version of SAE J183, “Engine Oil Performance and Engine Service Classification (Other than “Energy Conserving”)” API Publication 1509, “Engine Oil Licensing and Certification System,” European Automobile Manufacturers Association (ACEA), “European Oil Sequences,” or other “Vehicle or Engine Manufacturer Standards” as provided in Section 3.13.1.3.1.

(Amended 2012 and 2014)

* + - * 1. **Vehicle or Engine Manufacturer Standard. –** The label on any vehicle engine (motor) oil container, receptacle, dispenser, or storage tank and the invoice or receipt from service on an engine that includes the installation of vehicle engine (motor) oil dispensed from a receptacle, dispenser, or storage tank shall identify the specific vehicle or engine manufacturer standard, or standards, met in letters not less than 3.18 mm (1/8 in) in height. If the vehicle (motor) oil only meets a vehicle or engine manufac- turer standard, the label must clearly identify that the oil is only intended for use where specifically recommended by the vehicle or engine manufacturer.

(Added 2014)

* + - * 1. **Inactive or Obsolete Service Categories.** – The label on any vehicle engine (motor) oil container, receptacle, dispenser, or storage tank and the invoice or receipt from service on an engine that includes the installation of vehicle engine (motor) oil dispensed from a receptacle, dispenser, or storage tank shall bear a plainly visible cautionary statement in compliance with the latest version of SAE J183, “Engine Oil Performance and Engine Service Classification (Other than “Energy Conserving”)” Appen- dix A, whenever the vehicle engine (motor) oil in the container or in bulk does not meet an active API service category as defined by the latest version of SAE J183, “Engine Oil Performance and Engine Service Classification (Other than “Energy Conserving”).” If a vehicle engine (motor) oil is identified as only meeting a vehicle or engine manufacturer standard, the labeling requirements in Section 3.13.1.3.1. Vehicle or Engine Manufacturer Standard applies.

(Added 2012) (Amended 2014)

* + - 1. **Tank Trucks or Rail Cars.** – Tank trucks, rail cars, and types of delivery trucks that are used to deliver bulk vehicle engine (motor) oil are not required to display the SAE viscosity grade and service cate- gory or categories on such tank trucks, rail cars, and other types of delivery trucks.

(Added 2012) (Amend 2013 and 2014)

G. Uniform Fuels and Automotive Lubricants Regulation

* + - 1. **Documentation.** – When the engine (motor) oil is sold in bulk, an invoice, bill of lading, shipping paper, or other documentation must accompany each delivery. This document must identify the quantity of bulk engine (motor) oil delivered as defined in Sections 3.13.1.1. Viscosity; 3.13.1.2. Brand; 3.13.1.3. Engine Service Category; the name and address of the seller and buyer; and the date and time of the sale. For inactive or obsolete service categories, the documentation shall also bear a plainly visible cautionary statement as required in Section 3.13.1.3.2. Inactive or Obsolete Service Categories. Documentation must be retained at the retail establishment for a period of not less than one year.

(Added 2013) (Amended 2014)

(Amended 2012, 2013, and 2014)

## Labeling of Recreational Motor Oil.

* + - 1. **Viscosity.** – The label on each container of recreational motor oil shall contain the viscosity grade classification preceded by the letters “SAE” in accordance with the SAE International’s latest version of SAE J300, “Engine Oil Viscosity Classification.”
      2. **Intended Use.** – The label on each container of recreational motor oil shall contain a statement of its intended use in accordance with the latest version of SAE J300, “Engine Oil Viscosity Classification.”

## Labeling of Gear Oil.

* + - 1. **Viscosity.** – The label on each container of gear oil shall contain the viscosity grade classification preceded by the letters “SAE” in accordance with the SAE International’s latest version of SAE J306, “Au- tomotive Gear Lubricant Viscosity Classification” or SAE J300, “Engine Oil Viscosity Classification.”
         1. **Exception.** – Some automotive equipment manufacturers may not specify an SAE viscosity grade requirement for some applications. Gear oils intended to be used only in such applications are not required to contain an SAE viscosity grade on their labels.
      2. **Service Category.** – The label on each container of gear oil shall contain the service category, or categories, in letters not less than 3.18 mm (1/8 in) in height, as defined by the latest version of SAE J308, “Axle and Manual Transmission Lubricants.”

(Added 2004)

## Transmission Fluid.

* + 1. **Labeling and Identification of Transmission Fluid.** – Transmission fluid shall be labeled or identified as described below.

(Added 2017)

* + - 1. **Container Labeling.** – The label on a container of transmission fluid shall not contain any infor- mation that is false or misleading. Containers include bottles, cans, multi-quart or liter containers, pails, kegs, drums, and intermediate bulk containers (IBCs). In addition, each container of transmission fluid shall be labeled with the following:
         1. the brand name;
         2. the name and place of business of the manufacturer, packer, seller, or distributor;
         3. the words “Transmission Fluid,” which may be incorporated into a more specific description of transmission type such as “Automatic Transmission Fluid” or “Continuously Variable Transmission Fluid”;

G. Uniform Fuels and Automotive Lubricants Regulation

* + - * 1. the primary performance claim or claims met by the fluid and reference to where any supplemental claims may be viewed (e.g., website reference). Performance claims include but are not limited to those set by original equipment manufacturers and standards setting organizations such as SAE and JASO and are acknowledged by reference; and
        2. an accurate statement of the quantity of the contents in terms of liquid measure. (Amended 2017)
      1. **Identification on Documentation.** – Transmission fluid sold in bulk shall be identified on the manufacturer, packer, seller or distributor invoice, bill of lading, shipping paper, or other documentation with the information listed below:
         1. the brand name;
         2. the name and place of business of the manufacturer, packer, seller, or distributor;
         3. the words “Transmission Fluid” which may be incorporated into a more specific description of transmission type such as “Automatic Transmission Fluid” or “Continuously Variable Transmission Fluid”;
         4. the primary performance claim or claims met by the fluid or reference to where these claims may be viewed (e.g., website reference). Performance claims include but are not limited to those set by original equipment manufacturers and standards-setting organizations such as SAE and JASO and are acknowledged by reference; and
         5. an accurate statement of the quantity of the contents in terms of liquid measure. (Added 2017)
      2. **Identification on Service Provider Documentation.** – Transmission fluid installed from a bulk tank at time of transmission service shall be identified on the customer invoice with the information listed below:
         1. the brand name;
         2. the name and place of business of the service provider;
         3. the words “Transmission Fluid” which may be incorporated into a more specific description of transmission type such as “Automatic Transmission Fluid” or “Continuously Variable Transmission Fluid”;
         4. the primary performance claim or claims met by the fluid or reference to where these claims may be viewed (e.g., website reference). Performance claims include but are not limited to those set by original equipment manufacturers and standards-setting organizations such as SAE and JASO and are acknowledged by reference; and
         5. an accurate statement of the quantity of the contents in terms of liquid measure. (Added 2017)
      3. **Bulk Delivery.** – When the transmission fluid is sold in bulk, an invoice, bill of lading, shipping paper, or other documentation must accompany each delivery. This document must identify the fluid as defined in Section 3.14.2. Container Labeling.

(Added 2017)

* + - 1. **Storage Tank Labeling.** – Each storage tank of transmission fluid shall be labeled with the fol- lowing:

G. Uniform Fuels and Automotive Lubricants Regulation

1. the brand name;
2. the primary performance claim or claims met by the fluid or reference to where these claims may be viewed (e.g., website reference). Performance claims include but are not limited to those set by original equipment manufacturers and standards-setting organizations such as SAE and JASO and are acknowledged by reference.

(Added 2017)

* + - 1. **Documentation of Claims Made Upon Product Label.** – Any manufacturer, packer, or distrib- utor of any product subject to this article and sold in this state shall provide, upon request of duly authorized representatives of the Director, credible documentation of any claim made upon their product label, including claims made on any website referenced by said label. If the product performance claims published by a blender and/or marketer are based on the claim(s) of one or more additive suppliers, documentation of the claims may be requested in confidence by a duly authorized representative of the Director. Supporting data may be supplied directly to the Director’s office by the additive supplier(s).

(Added 2004) (Amended 2017)

## Biodiesel and Biodiesel Blends.

* + 1. **Identification of Product.** – Biodiesel Blendstock shall be identified by the term “biodiesel” with the designation “B100” or “B99.”

(Amended 2018)

## Labeling of Retail Dispensers.

* + - 1. **Labeling of Grade Required.** – Biodiesel shall be identified by the grades No. 1-B S15 or No. 1-B S500, or No. 2-B S500.

(Amended 2018)

* + - 1. **Automotive Fuel Rating.** – Biodiesel and biodiesel blends shall be labeled with its automotive fuel rating in accordance with the FTC Automotive Fuel Ratings, Certification and Posting Rule, 16 CFR 306.

(Amended 2018)

* + - 1. **Biodiesel Blends.** – When biodiesel blends greater than 20 % by volume are offered by sale, each side of the dispenser where fuel can be delivered shall have a label conspicuously placed that states “Consult Vehicle Manufacturer Fuel Recommendations.”

The lettering of this legend shall not be less than 6 mm (1/4 in) in height by 0.8 mm (1/32 in) stroke; block style letters and the color shall be in definite contrast to the background color to which it is applied.

* + 1. **Documentation for Dispenser Labeling Purposes.** – The retailer shall be provided, at the time of de- livery of the fuel, a declaration of the volume percent biodiesel on an invoice, bill of lading, shipping paper, or other document. This documentation is for dispenser labeling purposes only; it is the responsibility of any poten- tial blender to determine the amount of biodiesel in the diesel fuel prior to blending.
    2. **Exemption.** – Biodiesel blends that contain less than or equal to 5 % biodiesel by volume are exempted from the requirements of Sections 3.15.1. Identification of Product, 3.15.2. Labeling of Retail Dispensers, and

3.15.3. Documentation for Dispenser Labeling Purposes when it is sold as “diesel fuel” as required in Section 3.3. Diesel Fuel.

(Added 2005) (Amended 2008 and 2018)

G. Uniform Fuels and Automotive Lubricants Regulation

## Diesel Exhaust Fluid (DEF).

* + 1. **Labeling of Diesel Exhaust Fluid (DEF).** – DEF shall be labeled.
       1. **Retail Dispenser Labeling.** – A label shall be clearly and conspicuously placed on the front panel of the DEF dispenser stating “for operation of selective catalytic reduction (SCR) converters in motor vehi- cles with diesel engines.”
       2. **Documentation for Retailers of Bulk Product.** – A DEF supplier shall provide, at the time of delivery of the bulk shipment of DEF, identification of the fluid’s origin including the name of the fluid manufacturer, the brand name, trade name, or trademark, and a statement identifying the fluid as DEF con- forming to specifications given in the latest version of ISO 22241, “Diesel engines – NOx reduction agent AUS 32.” This information shall be provided by the supplier on an invoice, bill of lading, shipping paper, or other document.
       3. **Labeling Packaged Product.** – Any DEF retail package shall bear a label that includes the name of the fluid manufacturer, the brand name, trade name, or trademark, a statement identifying the fluid as DEF conforming to specifications given in the latest version of ISO 22241, “Diesel engines – NOx reduction agent AUX 32.” And the statement, “It is recommended to store DEF between − 5 °C to 30 °C (23 °F to 86 °F).”
       4. **Documentation for Bulk Deliveries.** – A carrier that transports or accepts for transportation any bulk shipment by tank truck, freight container, cargo tank, railcar, or any other vehicle used to transport or deliver bulk quantities of DEF shall, at the time of delivery of the DEF, provide identification of the fluid’s origin including the name of the fluid manufacturer, the brand name, trade name, or trademark, and a state- ment identifying the fluid as DEF conforming to specifications given in the latest version of ISO 22241, “Diesel engines – NOx reduction agent AUS 32.” This information shall be provided to the recipient on an invoice, bill of lading, shipping paper, or other document.

Effective date shall be January 1, 2016. (Added 2014)

## Tractor Hydraulic Fluid

* + 1. **Labeling and Identification of Tractor Hydraulic Fluid.** – Tractor hydraulic fluid shall be labeled or identified as described below
       1. **Container Labeling** – The label on a container of tractor hydraulic fluid shall not contain any information that is false or misleading. Containers include bottles, cans, multi-quart or liter containers, pails, kegs, drums, and intermediate bulk containers (IBCs). In addition, each container of tractor hydraulic fluid shall be labeled with the following:
          1. the brand name;
          2. the name and place of business of the manufacturer, packer, seller, or distributor;
          3. the words “Tractor Hydraulic Fluid,” which may include words such as “Hydraulic Fluid for Agri- cultural Applications” or “Universal Tractor Transmission Oil”;
          4. the primary performance claim or claims met by the fluid and reference to where any supplemental claims may be viewed (e.g., website reference). Performance claims are those set by original equip- ment manufacturers;
          5. any obsolete equipment manufacturer specifications should be clearly identified as “obsolete” and accompanied by the following warning on the front package label in clearly legible font size and color:

G. Uniform Fuels and Automotive Lubricants Regulation

**Caution:** Some specifications are no longer deemed active by the original equipment manufacturer. Significant harm to the transmission, hydraulic system, seals, final drive or axles is possible when using in applications in which it was not intended.

The above warning is not required if the fluid claims to meet current original equipment manufac- turer’s specifications and refers to thereby preceding specifications.

* + - * 1. an accurate statement of the quantity of the contents in terms of liquid measure.
      1. **Identification on Documentation.** – Tractor hydraulic fluid sold in bulk shall be identified on the manufacturer, packer, seller or distributor invoice, bill of lading, shipping paper, or other documentation with the information listed below:
         1. the brand name;
         2. the name and place of business of the manufacturer, packer, seller, or distributor;
         3. the words “Tractor Hydraulic Fluid,” which may include words such as “Hydraulic Fluid for Agri- cultural Applications” or “Universal Tractor Transmission Oil”;
         4. the primary performance claim or claims met by the fluid and reference to where any supplemental claims may be viewed (e.g., website reference). Performance claims include but are not limited to those set by original equipment manufacturers;
         5. any obsolete equipment manufacturer standard should be clearly identified as “obsolete” and ac- companied by the following warning on the front package label in clearly legible font size and color:

**Caution:** Some of the specifications are no longer deemed active by the original equipment manu- facturer. Significant harm to the transmission, hydraulic system, seals, final drive or axles is possible when using in applications in which it is not intended.

* + - * 1. The above warning is not required if the fluid claims to meet current original equipment manufac- turer’s specifications and refers to thereby preceding specifications.an accurate statement of the quantity of the contents in terms of liquid measure.
      1. **Identification on Service Provider Documentation.** – Tractor hydraulic fluid installed from a bulk tank at time of service shall be identified on the customer invoice with the information listed below:
         1. the brand name;
         2. the name and place of business of the service provider;
         3. the words “Tractor Hydraulic Fluid,” which may include words such as “Hydraulic Fluid for Agri- cultural Applications” or “Universal Tractor Transmission Oil”;
         4. the primary claim or claims met by the fluid and reference to where any supplemental claims may be viewed (e.g., website reference). Performance claims are those set by original equipment manu- facturers;
         5. any obsolete equipment manufacturer specifications should be clearly identified as “obsolete” and accompanied by the following warning on the front package label in clearly legible font size and color:

G. Uniform Fuels and Automotive Lubricants Regulation

**Caution:** Some of the specifications are no longer deemed active by the original equipment manu- facturer. Significant harm to the transmission, hydraulic system, seals, final drive or axles is possible when using in applications in which it is not intended.

The above warning is not required if the fluid claims to meet current original equipment manufac- turer’s specifications and refers to thereby preceding specifications.

* + - * 1. an accurate statement of the quantity of the contents in terms of liquid measure.
      1. **Bulk Delivery.** – When the tractor hydraulic fluid is sold in bulk, an invoice, bill of lading, shipping paper, or other documentation must accompany each delivery. This document must identify the fluid as defined in Section 3.17.1.1. Container Labeling.
      2. **Storage Tank Labeling.** – Each storage tank of tractor hydraulic fluid shall be labeled with the following:
         1. the brand name;
         2. the primary performance claim or claims met by the fluid and reference to where any supplemental claims may be viewed (e.g., website reference). Performance claims are those set by original equip- ment manufacturers;
      3. **Documentation of Claims Made Upon Product Label.** – Any manufacturer, packer, or distributor of any product subject to this article and sold shall provide, upon request of duly authorized representatives of the Director, credible documentation of any claim made upon their product label, including claims made on any website referenced by said label. If the product performance claims published by blender and/or marketer are based on the claim(s) of one or more additive suppliers, documentation of the claims shall be provided upon request to a duly authorized representative of the Director. Supporting data shall, upon re- quest, be supplied directly to the Director’s office by the additive supplier(s).

(Added 2019)

# Section 4. Retail Storage Tanks and Dispenser Filters

* 1. **Water in Gasoline-Alcohol Blends, Biodiesel Blends, Ethanol Flex Fuel, Aviation Gasoline, and Aviation Turbine Fuel.** – No water phase greater than 6 mm (¼ in) as determined by an appropriate detection paste or other acceptable means, is allowed to accumulate in any tank utilized in the storage of gasoline-alcohol blend, biodiesel, biodiesel blends, ethanol flex fuel, aviation gasoline, and aviation turbine fuel.

(Amended 2008, 2012, and 2014)

* 1. **Water in Gasoline, Diesel, Gasoline-Ether, and Other Fuels.** – Water shall not exceed 25 mm (1 in) in depth when measured with water indicating paste or other acceptable means in any tank utilized in the storage of diesel, gasoline, gasoline-ether blends, and kerosene sold at retail except as required in Section 4.1. Water in Gasoline-Alco- hol Blends, Biodiesel Blends, Ethanol Flex Fuel, Aviation Gasoline, and Aviation Turbine Fuel.

(Amended 2008, 2012, and 2014)

## Dispenser Filters.

## Engine Fuel Dispensers.

* + - 1. All gasoline, gasoline-alcohol blends, gasoline-ether blends, ethanol flex fuel, and M85 methanol dis- pensers shall have a 10 micron or smaller nominal pore-sized filter.

G. Uniform Fuels and Automotive Lubricants Regulation

This document is available free of charge from: https://doi.org/10.6028/NIST.HB.130-2020

* + - 1. All biodiesel, biodiesel blends, diesel, and kerosene dispensers shall have a 30 micron or smaller nominal pore-sized filter.

(Amended 2014)

## Delivery of Aviation Fuel and Gasoline.

* + - 1. Fuel delivery of aviation turbine fuel into aircraft shall be filtered through a fuel filter/separator con- forming to EI 1581, “Specification and Laboratory Qualification Procedures for Aviation Jet Fuel Fil- ter/Water Separators.”
      2. Fuel delivery of aviation gasoline into aircraft shall be filtered through a fuel filter/separator conforming to EI 1581, “Specification and Laboratory Qualification Procedures for Aviation Jet Fuel Filter/Water Separators.”

(Amended 2018)

(Added 2008) (Amended 2014 and 2018)

## Product Storage Identification.

* + 1. **Fill Connection Labeling.** – The fill connection for any fuel product storage tank or vessel supplying engine-fuel devices shall be permanently, plainly, and visibly marked as to the product contained.

(Amended 2008)

* + 1. **Declaration of Meaning of Color Code.** – When the fill connection device is marked by means of a color code, the color code shall be conspicuously displayed at the place of business and the API color codes as specified and published in “API Recommended Practice 1637” shall be used.

(Amended 2018)

* 1. **Volume of Product Information.** – Each retail location shall maintain on file a calibration chart or other means of determining the volume of each regulated product in each storage tank and the total capacity of such storage tank(s). This information shall be supplied immediately to the Director.

# Section 5. Condemned Product

* 1. **Stop-Sale Order at Retail.** – A stop-sale order may be issued to retail establishment dealers for fuels failing to meet specifications or when a condition exists that causes product degradation. A release from a stop-sale order will be awarded only after final disposition has been agreed upon by the Director. Confirmation of disposition shall be submitted in writing on form(s) provided by the Director and contain an explanation for the fuel’s failure to meet specifications. Upon discovery of fuels failing to meet specifications, meter readings and physical inventory shall be taken and reported in confirmation for disposition. Specific variations or exemptions may be made for fuels designed for special equipment or services and for which it can be demonstrated that the distribution will be restricted to those uses.
  2. **Stop-Sale Order at Terminal or Bulk Plant Facility.** – A stop-sale order may be issued when products main- tained at terminals or bulk plant facilities fail to meet specifications or when a condition exists that may cause product degradation. The terminal or bulk storage plant shall immediately notify all customers that received those product(s) and make any arrangements necessary to replace or adjust to specifications those product(s). A release from a stop- sale order will be awarded only after final disposition has been agreed upon by the Director. Confirmation of dispo- sition of products shall be made available in writing to the Director. Specific variations or exemptions may be made for fuels used for blending purposes or designed for special equipment or services and for which it can be demonstrated that the distribution will be restricted to those uses.

G. Uniform Fuels and Automotive Lubricants Regulation

# Section 6. Product Registration

* 1. **Engine Fuels Designed for Special Use.** – All engine fuels designed for special use that do not meet ASTM specifications or standards addressed in Section 2. Standard Specifications shall be registered with the Director on forms prescribed by the Director 30 days prior to when the registrant wishes to engage in sales. The registration form shall include all of the following information:
     1. **Identity.** – Business name and address(es).
     2. **Address.** – Mailing address, if different than business address.
     3. **Business Type.** – Type of ownership of the distributor or retail dealer, such as an individual, partnership, association, trust, corporation, or any other legal entity or combination thereof.
     4. **Signature.** – An authorized signature, title, and date for each registration.
     5. **Product Description.** – Product brand name and product description.
     6. **Product Specification.** – A product specification sheet shall be attached.
  2. **Renewal.** – Registration is subject to annual renewal.
  3. **Re-registration.** – Re-registration is required 30 days prior to any changes in Section 6.1. Engine Fuels De- signed for Special Use.
  4. **Authority to Deny Registration.** – The Director may decline to register any product that actually or by impli- cation would deceive or tend to deceive a purchaser as to the identity or the quality of the engine fuel.
  5. **Transferability.** – The registration is not transferable.

# Section 7. Test Methods and Reproducibility Limits

* 1. **ASTM Standard Test Methods.** – ASTM Standard Test Methods referenced for use within the applicable Standard Specification shall be used to determine the specification values for enforcement purposes.
     1. **Premium Diesel.** – The following test methods shall be used to determine compliance with the premium diesel parameters:
        1. **Cetane Number.** – The latest version of ASTM D613, “Standard Test Method for Cetane Number of Diesel Fuel Oil”;
        2. **Low Temperature Operability.** – The latest version of ASTM D4539, “Standard Test Method for Fil- terability of Diesel Fuels by Low-Temperature Flow Test (LTFT)” or ASTM D2500, “Standard Test Method for Cloud Point of Petroleum Products” (according to marketing claim);
        3. **Thermal Stability.** – The latest version of ASTM D6468, “Standard Test Method for High Temperature Stability of Middle Distillate Fuels” (180 min, 150 °C); and
        4. **Lubricity.** – The latest version of ASTM D6079, “Standard Test Method for Evaluating Lubricity of Diesel Fuels by the High Frequency Reciprocating Rig (HFRR).”

(Amended 2003)

G. Uniform Fuels and Automotive Lubricants Regulation

## Reproducibility Limits.

* + 1. **AKI Limits.** – When determining the antiknock index (AKI) acceptance or rejection of a gasoline sample, the AKI reproducibility limits as outlined in the latest version of ASTM D4814, “Standard Specification for Au- tomotive Spark-Ignition Engine Fuel,” Appendix X1 shall be acknowledged for enforcement purposes.
    2. **Reproducibility.** – The reproducibility limits of the standard test method used for each test performed shall be acknowledged for enforcement purposes, except as indicated in Section 2.2.1. Premium Diesel Fuel and Section 7.2.1. AKI Limits. No allowance shall be made for the precision of the test methods for aviation gasoline or aviation turbine fuels.

(Amended 2008)

* + 1. **SAE Viscosity Grades for Engine Oils.** – All values are critical specifications as defined in the latest version of ASTM D3244, “Standard Practice for Utilization of Test Data to Determine Conformance with Spec- ifications.” The product shall be considered to be in conformance if the Assigned Test Value (ATV) is within the specification.

(Added 2008)

* + 1. **Dispute Resolution.** – In the event of a dispute over a reported test value, the guidelines presented in the latest version of ASTM D3244, “Standard Practice for Utilization of Test Data to Determine Conformance with Specifications,” shall be used to determine the acceptance or rejection of the sample.
    2. **Additional Enforcement Action.** – The Director may initiate enforcement action in the event that, based upon a statistically significant number of samples, the average test result for products sampled from the same source location is greater than the legal maximum or less than the legal minimum limits (specification value), posted values, certified values, or registered values.

(Added 2008) (Amended 2018)

G. Uniform Fuels and Automotive Lubricants Regulation

THIS PAGE INTENTIONALLY LEFT BLANK