|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 2013 Amendments | | | | | |
| The following table lists the codes, paragraphs, and pages in which the 98th National Conference on Weights and Measures made amendments. In the column headed “Action,” changes are noted as “added,” “amended,” “deleted,” or “renumbered.” Each code, section, or paragraph that has been changed will be noted as “Added 2013” or “Amended 2013.” | | | | | |
| **SECTION** | **CODE** | **S&T**  **ITEM NO.** | **PARAGRAPH** | **ACTION** | **PAGE** |
| Introduction | L. Classifications for Agenda Items | BOD Item 120-4 | L. Classification for Agenda Items | Amended | 4 to 5 |
| M. Developing Items | Deleted and renumbered remaining items | 5 to 7 |
| 2.20. | Scales | 320-1 | S.6.4. | Amended | 2-25 |
| Table S.6.4.M. | Added | 2-26 |
| Table S.6.4. | Added | 2-26 |
| 2.21. | Belt-Conveyor Scale Systems | 321-1 | UR.1.2.(h) | Deleted and renumbered remaining subparagraphs | 2-69 to 2-70 |
| 3.30. | Liquid Measuring Devices | 330-2 | Table T.2. | Amended | 3-21 |
| 3.31. | Vehicle-Tank Meters | 331-1 | Table 1. | Amended | 3-40 |
| 331-2 | T.4. | Amended | 3-41 |
|  | Table T.4. | Deleted | 3-42 |
| 3.37. | Mass Flow Meters | 337-3 | Table T.2. | Amended | 3-112 |
| 5.56.(a) | Grain Moisture Meters | 356-1 | Table S.2.5. | Amended | 5-45 |
| 356-2 | UR.3.4. | Amended | 5-49 |
| Appendix C | General Tables of Units of Measurement | 320-4 | Units of Mass | Established uniform abbreviation for “short ton” and added footnote regarding effective dates. | C-6 |
| Avoirdupois Units of Mass | Established uniform abbreviation for “short ton” and added footnote regarding effective dates. | C-20 |
| Appendix D | Definitions | 320-1 | weigh module | Added | D-29 |
| 321-2 | belt load | Added | D-7 |
| belt revolution | Added | D-7 |
| integrator | Added | D-15 |
| loading point | Amended | D-16 |
| master weight totalizer | Amended | D-17 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **2013 Editorial Changes** | | | | | | |
| **SECTION** | | **CODE** | | **PARAGRAPH** | **ACTION** | **PAGE** |
| 2.21. | Belt-Conveyor Scales | | N.2.3. | | Replaced “(a)” and “(b)” in the latter section of the paragraph with “1.” and “2.” as in earlier editions of the handbook. | 2-65 |
| Appendix C | General Tables of Units of Measurement | | Units of Capacity or Volume – Liquid Volume Measurement | | Corrected milliliter equivalent of one gallon by deleting 3785.41 784 and replacing it with the correct value of 3785.411 784 milliliters. | C-12 |